<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<board>
<plain>
<text>+</text>
<text>+</text>
<text>+</text>
<text>PM2015</text>
<hole x="95" y="95" drill="4"/>
<hole x="5" y="25" drill="4"/>
<hole x="5" y="95" drill="4"/>
<text>Optional</text>
<text>QTouch</text>
<text>Optional</text>
<text>alimentare 12V</text>
<wire x1="30.518" y1="91.902" x2="30.518" y2="56.342" width="0.7" layer="46"/>
<wire x1="30.518" y1="56.342" x2="110.274" y2="55.342" width="0.7" layer="46"/>
<wire x1="110.274" y1="55.342" x2="110.274" y2="90.902" width="0.7" layer="46"/>
<wire x1="110.274" y1="90.902" x2="30.518" y2="91.902" width="0.7" layer="46"/>
<wire x1="38.392" y1="80.472" x2="38.392" y2="67.264" width="0.7" layer="46"/>
<wire x1="38.392" y1="67.264" x2="102.4" y2="67.264" width="0.7" layer="46"/>
<wire x1="102.4" y1="67.264" x2="102.4" y2="80.472" width="0.7" layer="46"/>
<wire x1="102.4" y1="80.472" x2="38.392" y2="80.472" width="0.7" layer="46"/>
<circle x="38.392" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="40.932" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="43.472" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="46.012" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="48.552" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="51.092" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="53.632" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="56.172" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="58.712" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="61.252" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="63.792" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="66.332" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="68.872" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<circle x="71.412" y="89.616" radius="0.359209375" width="0.7" layer="46"/>
<rectangle x1="41.55" y1="74.23" x2="44.49" y2="78.57" layer="46"/>
<rectangle x1="45.26" y1="74.2" x2="48.2" y2="78.54" layer="46"/>
<rectangle x1="48.86" y1="74.2" x2="51.8" y2="78.54" layer="46"/>
<rectangle x1="52.56" y1="74.2" x2="55.5" y2="78.54" layer="46"/>
<rectangle x1="41.56" y1="69.07" x2="44.5" y2="73.41" layer="46"/>
<rectangle x1="45.27" y1="69.04" x2="48.21" y2="73.38" layer="46"/>
<rectangle x1="48.87" y1="69.04" x2="51.81" y2="73.38" layer="46"/>
<rectangle x1="52.57" y1="69.04" x2="55.51" y2="73.38" layer="46"/>
<rectangle x1="56.1" y1="74.21" x2="59.04" y2="78.55" layer="46"/>
<rectangle x1="59.81" y1="74.18" x2="62.75" y2="78.52" layer="46"/>
<rectangle x1="63.41" y1="74.18" x2="66.35" y2="78.52" layer="46"/>
<rectangle x1="67.11" y1="74.18" x2="70.05" y2="78.52" layer="46"/>
<rectangle x1="56.11" y1="69.05" x2="59.05" y2="73.39" layer="46"/>
<rectangle x1="59.82" y1="69.02" x2="62.76" y2="73.36" layer="46"/>
<rectangle x1="63.42" y1="69.02" x2="66.36" y2="73.36" layer="46"/>
<rectangle x1="67.12" y1="69.02" x2="70.06" y2="73.36" layer="46"/>
<rectangle x1="70.82" y1="74.23" x2="73.76" y2="78.57" layer="46"/>
<rectangle x1="74.53" y1="74.2" x2="77.47" y2="78.54" layer="46"/>
<rectangle x1="78.13" y1="74.2" x2="81.07" y2="78.54" layer="46"/>
<rectangle x1="81.83" y1="74.2" x2="84.77" y2="78.54" layer="46"/>
<rectangle x1="70.83" y1="69.07" x2="73.77" y2="73.41" layer="46"/>
<rectangle x1="74.54" y1="69.04" x2="77.48" y2="73.38" layer="46"/>
<rectangle x1="78.14" y1="69.04" x2="81.08" y2="73.38" layer="46"/>
<rectangle x1="81.84" y1="69.04" x2="84.78" y2="73.38" layer="46"/>
<rectangle x1="85.37" y1="74.21" x2="88.31" y2="78.55" layer="46"/>
<rectangle x1="89.08" y1="74.18" x2="92.02" y2="78.52" layer="46"/>
<rectangle x1="92.68" y1="74.18" x2="95.62" y2="78.52" layer="46"/>
<rectangle x1="96.38" y1="74.18" x2="99.32" y2="78.52" layer="46"/>
<rectangle x1="85.38" y1="69.05" x2="88.32" y2="73.39" layer="46"/>
<rectangle x1="89.09" y1="69.02" x2="92.03" y2="73.36" layer="46"/>
<rectangle x1="92.69" y1="69.02" x2="95.63" y2="73.36" layer="46"/>
<rectangle x1="96.39" y1="69.02" x2="99.33" y2="73.36" layer="46"/>
<hole x="95" y="25" drill="4"/>
<text>Optional</text>
<text>alimentare 3.3V</text>
<text>Header LCD 2x16</text>
<wire x1="5" y1="20" x2="95" y2="20" width="0" layer="20"/>
<wire x1="100" y1="25" x2="100" y2="95" width="0" layer="20"/>
<wire x1="95" y1="100" x2="5" y2="100" width="0" layer="20"/>
<text>PORTA</text>
<text>PORTC</text>
<text>PORTD</text>
<text>PORTB</text>
<text>SPI</text>
<text>QUARTZ</text>
<text>RESET</text>
<text>QTOUCH</text>
<text>BTN</text>
<text>LED</text>
<text>PWR</text>
<wire x1="0" y1="95" x2="0" y2="25" width="0" layer="20"/>
<wire x1="0" y1="25" x2="5" y2="20" width="0" layer="20" curve="90"/>
<wire x1="95" y1="20" x2="100" y2="25" width="0" layer="20" curve="90"/>
<wire x1="0" y1="95" x2="5" y2="100" width="0" layer="20" curve="-90"/>
<text>D:/Downloads/logo.bmp</text>
<text>PM</text>
<text>SLIDER</text>
<text>FTDI</text>
<text>ALIM 3.3V</text>
<text>12V</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>Header LCD 2x16</text>
<text>PORTA</text>
<text>PORTC</text>
<text>PORTD</text>
<text>PORTB</text>
<text>SPI</text>
<text>QUARTZ</text>
<text>RESET</text>
<text>QTOUCH</text>
<text>BTN</text>
<text>LED</text>
<text>PWR</text>
<text>PM</text>
<text>SLIDER</text>
<text>FTDI</text>
<text>ALIM 3.3V</text>
<text>12V</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>C5</text>
<text>10u</text>
<text>C6</text>
<text>100nF</text>
<text>C7</text>
<text>100nF</text>
<text>C8</text>
<text>100nF</text>
<text>C10</text>
<text>100nF</text>
<text>C11</text>
<text>10u</text>
<text>C13</text>
<text>15pF</text>
<text>C15</text>
<text>15pF</text>
<text>D1</text>
<text>3V3</text>
<text>D2</text>
<text>IC1</text>
<text>LE33</text>
<text>IC2</text>
<text>MEGA324-P</text>
<text>IC3</text>
<text>7805</text>
<text>J1</text>
<text>J2</text>
<text>J3</text>
<text>JP1</text>
<text>JP3</text>
<text>Q1</text>
<text>R1</text>
<text>1k</text>
<text>R4</text>
<text>10k</text>
<text>R5</text>
<text>100</text>
<text>R6</text>
<text>100</text>
<text>R7</text>
<text>1k</text>
<text>R8</text>
<text>2K2</text>
<text>R9</text>
<text>100</text>
<text>R10</text>
<text>100</text>
<text>R11</text>
<text>100</text>
<text>R12</text>
<text>1K</text>
<text>R13</text>
<text>1K</text>
<text>R14</text>
<text>100</text>
<text>R15</text>
<text>10K</text>
<text>S1</text>
<text>S2</text>
<text>SJ1</text>
<text>SJ2</text>
<text>U1</text>
<text>FT231XS</text>
<wire x1="95.1" y1="100" x2="100.1" y2="95" width="0" layer="20" curve="-90"/>
</plain>
<libraries>
<library name="atmel">
<packages>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<packages>
<package name="MA10-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA03-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="special">
<packages>
<package name="QS">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="C025-025X050@1">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO34Z7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 1.8 mm, horizontal, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="0andrei_custom">
<packages>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="SJUMPER_PACK">
</package>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
<package name="LCD-16X2_NOSILK">
</package>
<package name="TO92">
<description>&lt;b&gt;TO-92&lt;/b&gt;</description>
</package>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="ZX62D-B-5PA8">
</package>
<package name="SSOP20">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
<package name="QT_SLIDER">
</package>
<package name="TO22H_NOHOLE">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="POWER_JACK_PTH_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-3-2-07">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="SJ-NC">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC2" library="atmel" package="DIL40" value="MEGA324-P">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="ATMEGA16-16PU"/>
<attribute name="OC_FARNELL" value="9171142"/>
<attribute name="OC_NEWARK" value="01M6885"/>
</element>
<element name="PORTD" library="con-lstb" package="MA10-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="special" package="QS" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="0andrei_custom" package="AVR-ISP-6" value="AVR-ISP-6">
<attribute name="NAME"/>
</element>
<element name="D1" library="diode" package="DO34Z7" value="3V3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="DO34Z7" value="3V3">
<attribute name="NAME"/>
</element>
<element name="R5" library="0andrei_custom" package="0204/7" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="0andrei_custom" package="0204/7" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="0andrei_custom" package="0204/7" value="2K2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="0andrei_custom" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="0andrei_custom" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="0andrei_custom" package="C025-025X050" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="LED2" library="led" package="LED3MM" value="">
<attribute name="MF" value="VISHAY SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="1612437"/>
</element>
<element name="S2" library="SparkFun" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="LED1" library="led" package="LED3MM" value="">
<attribute name="MF" value="VISHAY SEMICONDUCTOR"/>
<attribute name="OC_FARNELL" value="1612437"/>
</element>
<element name="C10" library="resistor" package="C025-025X050@1" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="resistor" package="E2,5-5" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="0andrei_custom" package="0204/7" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="0andrei_custom" package="0204/7" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="0andrei_custom" package="TO22H_NOHOLE" value="7805">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="0andrei_custom" package="0204/7" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="0andrei_custom" package="0204/7" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="resistor" package="E2,5-5" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="0andrei_custom" package="SJUMPER_PACK" value="SJUMPER"/>
<element name="C15" library="0andrei_custom" package="C025-025X050" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="0andrei_custom" package="0204/7" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="0andrei_custom" package="0204/7" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="con-lstb" package="MA03-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORTA" library="con-lstb" package="MA10-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="POWER_JACK_PTH_LOCK" value="POWER_JACKPTH_LOCK">
<attribute name="NAME"/>
</element>
<element name="X1" library="0andrei_custom" package="LCD-16X2_NOSILK" value="LCD-16X2NOSILK"/>
<element name="PORTC" library="con-lstb" package="MA10-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="0andrei_custom" package="0204/7" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PORTB" library="con-lstb" package="MA10-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="0andrei_custom" package="TO92" value="LE33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="0andrei_custom" package="USB-B-PTH" value="USBPTH">
<attribute name="NAME"/>
</element>
<element name="J1" library="0andrei_custom" package="ZX62D-B-5PA8" value="USBMICROUSB">
<attribute name="NAME"/>
</element>
<element name="U1" library="0andrei_custom" package="SSOP20" value="FT231XS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="resistor" package="C0603" value="0.1uF"/>
<element name="R3" library="resistor" package="R0603" value="22"/>
<element name="R2" library="resistor" package="R0603" value="22"/>
<element name="C2" library="resistor" package="C0603" value="22pF"/>
<element name="C3" library="resistor" package="C0603" value="22pF"/>
<element name="C4" library="resistor" package="C0603" value="100nF"/>
<element name="C6" library="0andrei_custom" package="C025-025X050" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-3-2-07" package="SJ-NC" value="SOLDERJUMPERNC"/>
<element name="SJ2" library="SparkFun-3-2-07" package="SJ-NC" value="SOLDERJUMPERNC"/>
<element name="C9" library="resistor" package="C1206" value="27pF"/>
<element name="R10" library="resistor" package="M1206" value="100"/>
<element name="R11" library="resistor" package="M1206" value="100"/>
<element name="R14" library="resistor" package="M1206" value="100"/>
<element name="C12" library="resistor" package="C1206" value="27pF"/>
<element name="C14" library="resistor" package="C1206" value="27pF"/>
<element name="U$1" library="0andrei_custom" package="QT_SLIDER" value="QT_SLIDER"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="6"/>
<contactref element="PORTD" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="IC2" pad="11"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="IC2" pad="31"/>
<contactref element="C13" pad="1"/>
<contactref element="C11" pad="-"/>
<contactref element="C10" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="IC3" pad="2"/>
<contactref element="S1" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C5" pad="-"/>
<contactref element="LED2" pad="K"/>
<contactref element="C15" pad="1"/>
<contactref element="PORTA" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="PORTC" pad="1"/>
<contactref element="PORTB" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="J2" pad="GND"/>
<contactref element="J1" pad="GND"/>
<contactref element="J1" pad="P$10"/>
<contactref element="J1" pad="P$8"/>
<contactref element="J1" pad="P$11"/>
<contactref element="J1" pad="P$9"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="16"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="J3" pad="GNDBREAK"/>
<contactref element="J3" pad="GND"/>
<contactref element="LED1" pad="K"/>
<contactref element="C6" pad="2"/>
<contactref element="J2" pad="P$1"/>
<contactref element="J2" pad="P$2"/>
</signal>
<signal name="PD1">
<contactref element="IC2" pad="15"/>
<contactref element="PORTD" pad="9"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="PD0">
<contactref element="IC2" pad="14"/>
<contactref element="PORTD" pad="10"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="+5V">
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="PB6">
<contactref element="JP1" pad="1"/>
<contactref element="IC2" pad="7"/>
<contactref element="PORTB" pad="4"/>
</signal>
<signal name="PB5">
<contactref element="JP1" pad="4"/>
<contactref element="IC2" pad="6"/>
<contactref element="PORTB" pad="5"/>
</signal>
<signal name="PB7">
<contactref element="JP1" pad="3"/>
<contactref element="IC2" pad="8"/>
<contactref element="PORTB" pad="3"/>
</signal>
<signal name="PB4">
<contactref element="IC2" pad="5"/>
<contactref element="PORTB" pad="6"/>
</signal>
<signal name="PA7">
<contactref element="IC2" pad="33"/>
<contactref element="PORTA" pad="10"/>
</signal>
<signal name="PA6">
<contactref element="IC2" pad="34"/>
<contactref element="PORTA" pad="9"/>
</signal>
<signal name="PA5">
<contactref element="IC2" pad="35"/>
<contactref element="PORTA" pad="8"/>
</signal>
<signal name="PA4">
<contactref element="IC2" pad="36"/>
<contactref element="PORTA" pad="7"/>
</signal>
<signal name="PA3">
<contactref element="IC2" pad="37"/>
<contactref element="PORTA" pad="6"/>
</signal>
<signal name="PA2">
<contactref element="IC2" pad="38"/>
<contactref element="PORTA" pad="5"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="PA1">
<contactref element="IC2" pad="39"/>
<contactref element="PORTA" pad="4"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="PA0">
<contactref element="IC2" pad="40"/>
<contactref element="PORTA" pad="3"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="PB3">
<contactref element="IC2" pad="4"/>
<contactref element="PORTB" pad="7"/>
</signal>
<signal name="PB2">
<contactref element="IC2" pad="3"/>
<contactref element="PORTB" pad="8"/>
<contactref element="R14" pad="1"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="PB1">
<contactref element="IC2" pad="2"/>
<contactref element="PORTB" pad="9"/>
<contactref element="R11" pad="1"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="PB0">
<contactref element="IC2" pad="1"/>
<contactref element="PORTB" pad="10"/>
<contactref element="R10" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="PC7">
<contactref element="IC2" pad="29"/>
<contactref element="X1" pad="4"/>
<contactref element="R1" pad="1"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="PC6">
<contactref element="IC2" pad="28"/>
<contactref element="X1" pad="5"/>
<contactref element="PORTC" pad="4"/>
</signal>
<signal name="PC5">
<contactref element="IC2" pad="27"/>
<contactref element="X1" pad="6"/>
<contactref element="PORTC" pad="5"/>
</signal>
<signal name="PC4">
<contactref element="IC2" pad="26"/>
<contactref element="X1" pad="11"/>
<contactref element="PORTC" pad="6"/>
</signal>
<signal name="PC3">
<contactref element="IC2" pad="25"/>
<contactref element="X1" pad="12"/>
<contactref element="PORTC" pad="7"/>
</signal>
<signal name="PC2">
<contactref element="IC2" pad="24"/>
<contactref element="X1" pad="13"/>
<contactref element="PORTC" pad="8"/>
</signal>
<signal name="PC1">
<contactref element="IC2" pad="23"/>
<contactref element="X1" pad="14"/>
<contactref element="PORTC" pad="9"/>
</signal>
<signal name="PC0">
<contactref element="IC2" pad="22"/>
<contactref element="PORTC" pad="10"/>
</signal>
<signal name="PD7">
<contactref element="IC2" pad="21"/>
<contactref element="PORTD" pad="3"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="PD6">
<contactref element="IC2" pad="20"/>
<contactref element="PORTD" pad="4"/>
<contactref element="S2" pad="4"/>
<contactref element="S2" pad="3"/>
</signal>
<signal name="PD5">
<contactref element="IC2" pad="19"/>
<contactref element="PORTD" pad="5"/>
</signal>
<signal name="PD4">
<contactref element="IC2" pad="18"/>
<contactref element="PORTD" pad="6"/>
</signal>
<signal name="PD3">
<contactref element="IC2" pad="17"/>
<contactref element="PORTD" pad="7"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="PD2">
<contactref element="IC2" pad="16"/>
<contactref element="PORTD" pad="8"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R6" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="J2" pad="D+"/>
</signal>
<signal name="N$15">
<contactref element="R5" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="J2" pad="D-"/>
</signal>
<signal name="N$20">
<contactref element="IC2" pad="32"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="C13" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="N$22">
<contactref element="IC2" pad="12"/>
<contactref element="Q1" pad="1"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="C10" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="J3" pad="PWR"/>
</signal>
<signal name="N$18">
<contactref element="IC3" pad="3"/>
<contactref element="C11" pad="+"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$17">
<contactref element="S2" pad="2"/>
<contactref element="S2" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="IC2" pad="9"/>
<contactref element="S1" pad="3"/>
<contactref element="S1" pad="4"/>
<contactref element="R15" pad="1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="R11" pad="2"/>
<contactref element="U$1" pad="CHAN1"/>
</signal>
<signal name="VCC">
<contactref element="R7" pad="2"/>
<contactref element="IC2" pad="30"/>
<contactref element="C7" pad="1"/>
<contactref element="IC2" pad="10"/>
<contactref element="C8" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="PORTD" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="PORTA" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="PORTC" pad="3"/>
<contactref element="PORTB" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="C5" pad="+"/>
<contactref element="JP2" pad="3"/>
<contactref element="IC1" pad="3"/>
<contactref element="U1" pad="15"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="14"/>
<contactref element="C1" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED2" pad="A"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="VBUS">
<contactref element="JP3" pad="1"/>
<contactref element="J2" pad="VBUS"/>
<contactref element="SJ2" pad="1"/>
</signal>
<signal name="A">
<contactref element="X1" pad="15"/>
</signal>
<signal name="K">
<contactref element="X1" pad="16"/>
</signal>
<signal name="VO">
<contactref element="X1" pad="3"/>
<contactref element="R4" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="PORTC" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="DM">
<contactref element="J1" pad="D-"/>
<contactref element="R3" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="DP">
<contactref element="J1" pad="D+"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="TXLED">
<contactref element="U1" pad="10"/>
</signal>
<signal name="FTD_N">
<contactref element="U1" pad="12"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="FTD_P">
<contactref element="U1" pad="11"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RXLED">
<contactref element="U1" pad="17"/>
</signal>
<signal name="N$2">
<contactref element="R12" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="VBUS"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R14" pad="2"/>
<contactref element="U$1" pad="CHAN0"/>
</signal>
<signal name="N$7">
<contactref element="R10" pad="2"/>
<contactref element="U$1" pad="CHAN2A"/>
<contactref element="U$1" pad="CHAN2B"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
