<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="102.09653125" y1="150" x2="-97.90346875" y2="150" width="0" layer="20"/>
<wire x1="-97.90346875" y1="150" x2="-97.90346875" y2="0" width="0" layer="20"/>
<wire x1="-97.90346875" y1="0" x2="102.09653125" y2="0" width="0" layer="20"/>
<wire x1="102.09653125" y1="0" x2="102.09653125" y2="150" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BUZZER-12MM">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Displays">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of display devices- LED displays, LCD displays, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LCD-G12864">
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA08-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA10-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92-AMMO">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE15">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ACTION" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="JOURNAL" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="MENU" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="INVENTORY" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="SKILLS" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="AUX" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="MAP" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="LEFT" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="SNEAK" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="SG2" library="SparkFun-Electromechanical" package="BUZZER-12MM" value="BUZZERPTH"/>
<element name="U$1" library="SparkFun-Displays" package="LCD-G12864" value="LCD-G12864FULL"/>
<element name="SV1" library="con-lsta" package="FE15" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="500"/>
<element name="Q2" library="SparkFun-DiscreteSemi" package="TO-92-AMMO" value=""/>
<element name="SV2" library="con-lstb" package="MA08-1" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="SV3" library="con-lstb" package="MA10-1" value="">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
</element>
<element name="R2" library="SparkFun-Resistors" package="R2010" value=""/>
<element name="UP" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="RIGHT" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
<element name="DOWN" library="SparkFun-Retired" package="TACTILE-PTH" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="LEFT" pad="1"/>
<contactref element="MENU" pad="2"/>
<contactref element="MENU" pad="1"/>
<contactref element="JOURNAL" pad="2"/>
<contactref element="JOURNAL" pad="1"/>
<contactref element="SKILLS" pad="2"/>
<contactref element="SKILLS" pad="1"/>
<contactref element="ACTION" pad="2"/>
<contactref element="ACTION" pad="1"/>
<contactref element="MAP" pad="2"/>
<contactref element="MAP" pad="1"/>
<contactref element="INVENTORY" pad="2"/>
<contactref element="INVENTORY" pad="1"/>
<contactref element="SNEAK" pad="2"/>
<contactref element="SNEAK" pad="1"/>
<contactref element="AUX" pad="2"/>
<contactref element="AUX" pad="1"/>
<contactref element="LEFT" pad="2"/>
<contactref element="SG2" pad="-"/>
<contactref element="U$1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="UP" pad="2"/>
<contactref element="UP" pad="1"/>
<contactref element="RIGHT" pad="2"/>
<contactref element="RIGHT" pad="1"/>
<contactref element="DOWN" pad="2"/>
<contactref element="DOWN" pad="1"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="LEFT" pad="3"/>
<contactref element="SV1" pad="11"/>
<contactref element="LEFT" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="SV1" pad="10"/>
<contactref element="AUX" pad="3"/>
<contactref element="AUX" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="SV1" pad="9"/>
<contactref element="SNEAK" pad="3"/>
<contactref element="SNEAK" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="SV1" pad="8"/>
<contactref element="INVENTORY" pad="3"/>
<contactref element="INVENTORY" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="MENU" pad="4"/>
<contactref element="MENU" pad="3"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="JOURNAL" pad="4"/>
<contactref element="SV1" pad="4"/>
<contactref element="JOURNAL" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="SKILLS" pad="4"/>
<contactref element="SV1" pad="5"/>
<contactref element="SKILLS" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="ACTION" pad="3"/>
<contactref element="ACTION" pad="4"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="N$12">
<contactref element="R1" pad="P$2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="Q2" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="SG2" pad="+"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="20"/>
<contactref element="SV3" pad="9"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="18"/>
<contactref element="SV3" pad="7"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="17"/>
<contactref element="SV3" pad="6"/>
</signal>
<signal name="N$19">
<contactref element="U$1" pad="16"/>
<contactref element="SV3" pad="5"/>
</signal>
<signal name="N$20">
<contactref element="U$1" pad="15"/>
<contactref element="SV3" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="14"/>
<contactref element="SV3" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="13"/>
<contactref element="SV3" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="12"/>
<contactref element="SV3" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="11"/>
<contactref element="SV2" pad="8"/>
</signal>
<signal name="N$25">
<contactref element="SV2" pad="7"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="9"/>
<contactref element="SV2" pad="6"/>
</signal>
<signal name="N$27">
<contactref element="SV2" pad="5"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="N$28">
<contactref element="U$1" pad="7"/>
<contactref element="SV2" pad="4"/>
</signal>
<signal name="N$29">
<contactref element="SV2" pad="3"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="N$30">
<contactref element="U$1" pad="5"/>
<contactref element="SV2" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="SV2" pad="1"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="SV1" pad="12"/>
<contactref element="UP" pad="4"/>
<contactref element="UP" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="MAP" pad="4"/>
<contactref element="SV1" pad="7"/>
<contactref element="MAP" pad="3"/>
</signal>
<signal name="N$11">
<contactref element="RIGHT" pad="4"/>
<contactref element="SV1" pad="13"/>
<contactref element="RIGHT" pad="3"/>
</signal>
<signal name="N$32">
<contactref element="DOWN" pad="4"/>
<contactref element="SV1" pad="14"/>
<contactref element="DOWN" pad="3"/>
</signal>
<signal name="N$33">
<contactref element="R1" pad="P$1"/>
<contactref element="SV1" pad="15"/>
</signal>
<signal name="N$34">
<contactref element="U$1" pad="19"/>
<contactref element="SV3" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
